(kicad_pcb (version 3) (host pcbnew "(2013-07-07 BZR 4022)-stable")

  (general
    (links 0)
    (no_connects 0)
    (area 8.849999 64.049999 290.550001 175.050001)
    (thickness 1.6)
    (drawings 21)
    (tracks 0)
    (zones 0)
    (modules 91)
    (nets 1)
  )

  (page A4)
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user)
    (25 Cmts.User user)
    (26 Eco1.User user)
    (27 Eco2.User user)
    (28 Edge.Cuts user)
  )

  (setup
    (last_trace_width 0.508)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.1)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.01)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.032 1.032)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFB3F)
    (pcbplotparams
      (layerselection 278953984)
      (usegerberextensions true)
      (excludeedgelayer false)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber20190414/cover8/))
  )

  (net 0 "")

  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
  )

  (net_class Strong ""
    (clearance 0.381)
    (trace_width 0.508)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )

  (module 1PIN_SMD (layer F.Cu) (tedit 5CD9B0D5) (tstamp 5CDA6C90)
    (at 286.5 128.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path 1pin)
    (fp_text reference 1PIN_SMD (at 0 -3.50012) (layer F.SilkS) hide
      (effects (font (size 1.016 1.016) (thickness 0.254)))
    )
    (fp_text value P*** (at 0.24892 3.74904) (layer F.SilkS) hide
      (effects (font (size 1.016 1.016) (thickness 0.254)))
    )
    (pad 1 smd rect (at 0 0) (size 2.032 1.032)
      (layers F.Cu F.Paste F.SilkS F.Mask)
    )
  )

  (module 1PIN_SMD (layer F.Cu) (tedit 5CD9B061) (tstamp 5CDA6C02)
    (at 283.5 128.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path 1pin)
    (fp_text reference 1PIN_SMD (at 0 -3.50012) (layer F.SilkS) hide
      (effects (font (size 1.016 1.016) (thickness 0.254)))
    )
    (fp_text value P*** (at 0.24892 3.74904) (layer F.SilkS) hide
      (effects (font (size 1.016 1.016) (thickness 0.254)))
    )
    (pad 1 smd rect (at 0 0) (size 2.032 1.032)
      (layers F.Cu F.Paste F.SilkS F.Mask)
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F22E4)
    (at 169 99.8)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF5B2)
    (fp_text reference DMB9 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F22CB)
    (at 179 99.8)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF5B8)
    (fp_text reference DMB10 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F22B2)
    (at 189 99.8)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF5BE)
    (fp_text reference DMB11 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F2299)
    (at 199 99.8)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF5C4)
    (fp_text reference DMB12 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F2280)
    (at 89 114.4)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF5CC)
    (fp_text reference DAC1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F2267)
    (at 99 114.4)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF5E5)
    (fp_text reference DAC2 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F224E)
    (at 109 114.4)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF5EB)
    (fp_text reference DAC3 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F2235)
    (at 119 114.4)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF5F1)
    (fp_text reference DAC4 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F221C)
    (at 129 114.4)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF5F7)
    (fp_text reference DAC5 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F2203)
    (at 139 114.4)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF5FD)
    (fp_text reference DAC6 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F21EA)
    (at 149 114.4)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF603)
    (fp_text reference DAC7 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F21D1)
    (at 159 114.4)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF609)
    (fp_text reference DAC8 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F21B8)
    (at 169 114.4)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF60F)
    (fp_text reference DAC9 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F219F)
    (at 179 114.4)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF615)
    (fp_text reference DAC10 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F2186)
    (at 89 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF34A)
    (fp_text reference DPC1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F216D)
    (at 199 114.4)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF621)
    (fp_text reference DAC12 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F2154)
    (at 89 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF629)
    (fp_text reference DMQ1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F213B)
    (at 99 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF642)
    (fp_text reference DMQ2 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F2122)
    (at 109 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF648)
    (fp_text reference DMQ3 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F2109)
    (at 119 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF64E)
    (fp_text reference DMQ4 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F20F0)
    (at 129 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF654)
    (fp_text reference DMQ5 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F20D7)
    (at 139 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF65A)
    (fp_text reference DMQ6 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F20BE)
    (at 149 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF660)
    (fp_text reference DMQ7 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F20A5)
    (at 159 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF666)
    (fp_text reference DMQ8 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F208C)
    (at 169 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF66C)
    (fp_text reference DMQ9 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F2073)
    (at 179 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF672)
    (fp_text reference DMQ10 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F205A)
    (at 189 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF678)
    (fp_text reference DMQ11 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F2041)
    (at 199 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF67E)
    (fp_text reference DMQ12 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F2028)
    (at 79 114.4)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF686)
    (fp_text reference DLINK1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F200F)
    (at 29 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF6A1)
    (fp_text reference DSC1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1FF6)
    (at 189 114.4)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF61B)
    (fp_text reference DAC11 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1FDD)
    (at 99 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF399)
    (fp_text reference DPC2 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1FC4)
    (at 109 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF3AC)
    (fp_text reference DPC3 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1FAB)
    (at 119 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF3B2)
    (fp_text reference DPC4 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1F92)
    (at 129 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF3B8)
    (fp_text reference DPC5 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1F79)
    (at 139 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF3BE)
    (fp_text reference DPC6 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1F60)
    (at 149 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF3C4)
    (fp_text reference DPC7 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1F47)
    (at 159 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF3CA)
    (fp_text reference DPC8 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1F2E)
    (at 169 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF3D0)
    (fp_text reference DPC9 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1F15)
    (at 179 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF3D6)
    (fp_text reference DPC10 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1EFC)
    (at 189 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF3DC)
    (fp_text reference DPC11 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1EE3)
    (at 199 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF3E2)
    (fp_text reference DPC12 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1ECA)
    (at 89 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF463)
    (fp_text reference DMA1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1EB1)
    (at 99 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF47C)
    (fp_text reference DMA2 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1E98)
    (at 109 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF482)
    (fp_text reference DMA3 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1E7F)
    (at 159 99.8)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF5AC)
    (fp_text reference DMB8 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1E66)
    (at 129 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF48E)
    (fp_text reference DMA5 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1E4D)
    (at 139 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF494)
    (fp_text reference DMA6 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1E34)
    (at 149 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF49A)
    (fp_text reference DMA7 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1E1B)
    (at 159 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF4A0)
    (fp_text reference DMA8 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1E02)
    (at 169 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF4A6)
    (fp_text reference DMA9 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1DE9)
    (at 179 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF4AC)
    (fp_text reference DMA10 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1DD0)
    (at 189 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF4B2)
    (fp_text reference DMA11 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1DB7)
    (at 199 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF4B8)
    (fp_text reference DMA12 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1D9E)
    (at 89 99.8)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF56F)
    (fp_text reference DMB1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1D85)
    (at 99 99.8)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF588)
    (fp_text reference DMB2 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1D6C)
    (at 109 99.8)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF58E)
    (fp_text reference DMB3 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1D53)
    (at 119 99.8)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF594)
    (fp_text reference DMB4 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1D3A)
    (at 129 99.8)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF59A)
    (fp_text reference DMB5 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1D21)
    (at 139 99.8)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF5A0)
    (fp_text reference DMB6 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1D08)
    (at 149 99.8)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF5A6)
    (fp_text reference DMB7 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1CEF)
    (at 119 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF488)
    (fp_text reference DMA4 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1CD6)
    (at 279 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF843)
    (fp_text reference DRUN1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1CBD)
    (at 279 77.9)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF83D)
    (fp_text reference DPAUSE1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1CA4)
    (at 279 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF837)
    (fp_text reference DION1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1C8B)
    (at 259 107.1)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF7E9)
    (fp_text reference DBREAK1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1C72)
    (at 259 99.8)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF7E3)
    (fp_text reference DCURAD1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1C59)
    (at 259 92.5)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF7DD)
    (fp_text reference DWRDCT1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1C40)
    (at 259 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF7D7)
    (fp_text reference DDEFER1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1C27)
    (at 259 77.9)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF7D1)
    (fp_text reference DEXEC1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1C0E)
    (at 259 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF7CB)
    (fp_text reference DFETCH1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1BF5)
    (at 239 121.4)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF789)
    (fp_text reference DOPR1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1BDC)
    (at 239 114.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF783)
    (fp_text reference DIOT1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1BC3)
    (at 239 107)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF77D)
    (fp_text reference DJMP1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1BAA)
    (at 239 99.8)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF777)
    (fp_text reference DJMS1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1B91)
    (at 239 92.5)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF741)
    (fp_text reference DDCA1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1B78)
    (at 39 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF6BA)
    (fp_text reference DSC2 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1B5F)
    (at 59 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF6C6)
    (fp_text reference DSC4 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1B46)
    (at 69 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF6CC)
    (fp_text reference DSC5 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1B14)
    (at 29 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF6DA)
    (fp_text reference DDF1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1AFB)
    (at 39 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF6F3)
    (fp_text reference DDF2 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1AE2)
    (at 49 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF6F9)
    (fp_text reference DDF3 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1AC9)
    (at 49 129)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF6C0)
    (fp_text reference DSC3 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1AB0)
    (at 239 77.9)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF735)
    (fp_text reference DTAD1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1A97)
    (at 239 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF728)
    (fp_text reference DAND1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1A7E)
    (at 239 85.2)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF73B)
    (fp_text reference DISZ1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1A65)
    (at 69 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF71A)
    (fp_text reference DIF2 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1A4C)
    (at 79 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF720)
    (fp_text reference DIF3 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module PIDP8-LED-COVER (layer F.Cu) (tedit 5C1F8BDD) (tstamp 548F1A33)
    (at 59 70.6)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (path /548EF701)
    (fp_text reference DIF1 (at 0 -5.5372) (layer F.SilkS) hide
      (effects (font (size 0.7 0.7) (thickness 0.025)))
    )
    (fp_text value LED (at 0 2.54) (layer F.SilkS) hide
      (effects (font (size 0.762 0.762) (thickness 0.0889)))
    )
    (pad "" np_thru_hole circle (at 0 0) (size 5.03 5.03) (drill 4.85)
      (layers *.Cu F.Mask)
    )
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text PiDP-8 (at 285 127) (layer F.SilkS)
    (effects (font (size 0.8 0.9) (thickness 0.2)))
  )
  (gr_line (start 290 64.1) (end 290 65.3) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 19.6 64.1) (end 290 64.1) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 19.6 65.3) (end 19.6 64.1) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 19.6 121.5) (end 71.5 121.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 290 135.8) (end 290 65.8) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 19.6 135.8) (end 290 135.8) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 19.6 121.5) (end 19.6 135.8) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 19.6 78) (end 71.5 78) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 290 65.3) (end 290 65.8) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 19.6 65.8) (end 19.6 65.3) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 19.6 78) (end 19.6 65.8) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.5 78) (end 71.5 121.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 9.5 65.8) (end 8.9 65.8) (angle 90) (layer Dwgs.User) (width 0.1))
  (gr_line (start 9.5 65.2) (end 9.5 65.8) (angle 90) (layer Dwgs.User) (width 0.1))
  (gr_line (start 9.5 174.5) (end 9.5 174.9) (angle 90) (layer Dwgs.User) (width 0.1))
  (gr_line (start 9.1 174.5) (end 9.5 174.5) (angle 90) (layer Dwgs.User) (width 0.1))
  (gr_line (start 290 174.5) (end 290 175) (angle 90) (layer Dwgs.User) (width 0.1))
  (gr_line (start 290.5 174.5) (end 290 174.5) (angle 90) (layer Dwgs.User) (width 0.1))
  (gr_line (start 290 65.8) (end 290.4 65.8) (angle 90) (layer Dwgs.User) (width 0.1))
  (gr_line (start 290 65.4) (end 290 65.8) (angle 90) (layer Dwgs.User) (width 0.1))

)
