
(rules PCB PDP8
  (snap_angle 
    fortyfive_degree
  )
  (autoroute_settings
    (fanout off)
    (autoroute on)
    (postroute on)
    (vias on)
    (via_costs 50)
    (plane_via_costs 5)
    (start_ripup_costs 100)
    (start_pass_no 19938)
    (layer_rule F.Cu
      (active on)
      (preferred_direction horizontal)
      (preferred_direction_trace_costs 1.0)
      (against_preferred_direction_trace_costs 3.9)
    )
    (layer_rule B.Cu
      (active on)
      (preferred_direction vertical)
      (preferred_direction_trace_costs 1.0)
      (against_preferred_direction_trace_costs 1.3)
    )
  )
  (rule
    (width 254.0)
    (clear 254.2)
    (clear 127.0 (type smd_to_turn_gap))
    (clear 63.6 (type smd_smd))
  )
  (padstack "Via[0-1]_889:635_um"
    (shape
      (circle F.Cu 889.0 0.0 0.0)
    )
    (shape
      (circle B.Cu 889.0 0.0 0.0)
    )
    (attach off)
  )
  (padstack "Via[0-1]_889:0_um"
    (shape
      (circle F.Cu 889.0 0.0 0.0)
    )
    (shape
      (circle B.Cu 889.0 0.0 0.0)
    )
    (attach off)
  )
  (via 
    "Via[0-1]_889:635_um" "Via[0-1]_889:635_um" default
  )
  (via 
    "Via[0-1]_889:0_um" "Via[0-1]_889:0_um" default
  )
  (via 
    "Via[0-1]_889:635_um-kicad_default" "Via[0-1]_889:635_um" "kicad_default"
  )
  (via 
    "Via[0-1]_889:0_um-kicad_default" "Via[0-1]_889:0_um" "kicad_default"
  )
  (via_rule
    default "Via[0-1]_889:635_um"
  )
  (via_rule
    "kicad_default" "Via[0-1]_889:635_um-kicad_default"
  )
  (class default
    (clearance_class default)
    (via_rule default)
    (rule
      (width 254.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
  (class "kicad_default"
    "N-0000023" "N-0000028" "N-0000029" "N-0000035" "N-0000039" "N-0000040" "N-0000041" "N-0000042"
    "N-0000043" "N-0000046" "N-0000048" "N-0000049" "N-0000050" "N-0000053" "N-0000054" "N-0000055"
    "N-0000056" "N-0000057" "N-0000059" "N-0000060" "N-0000061" "N-0000062" "N-0000063" "N-0000065"
    "N-0000066" "N-0000067" "N-0000068" "N-0000069" "N-0000070" "N-0000071" "N-0000072" "N-0000073"
    "N-0000074" "N-0000079" "N-0000085" "N-0000086" "N-0000087" "N-0000088" "N-0000089" "N-0000090"
    "N-0000091" "N-0000092" "N-0000093" RX "SPARE_IO" TX col1 col10
    col11 col12 col1a col2 col2a col3 col4 col5
    col6 col7 col8 col9 led1 led2 led3 led4
    led5 led6 led7 led8 xled1 xled2 xled3 xled4
    xled5 xled6 xled7 xled8
    (clearance_class "kicad_default")
    (via_rule kicad_default)
    (rule
      (width 254.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
  (class fat
    +3.3V +5V GND row1 row2 row3
    (clearance_class default)
    (via_rule default)
    (rule
      (width 381.0)
    )
    (circuit 
      (use_layer F.Cu B.Cu)
    )
  )
)