# Install the final packages to our patched rk05 image
# to create the boot image we normally use.

copy $os8mo/v3d-patched.rk05 $os8mo/v3d.rk05
mount rk0 $os8mo/v3d.rk05 required

boot rk0

# Include our dynamically specified packages.
include $build/obj/os8pkg/pkgs.os8

# Squish our device as our last step!

os8 SQUISH DSK:/O
os8 SQUISH SYS:/O
