# IOTABLE OVERFLOW (SPR 8-2431 JR)
# Problem: The size of the IOTABLE is 15 (Octal).
# This was misread as 15 (Decimal) making entry #4 overflow into the handler.
# 
# The following patch will fix the problem and upgrades BRTS.SV to V5B.

.GET SYS BRTS
.ODT
2010/ 7106 7104\n
2011/ 7006 1065\n
2012/ 7041 7006\n
2013/ 1065 1065\n
2014/ 7041 7000
1116/ 0301 0302
\c
.SAVE SYS BRTS
