# Script to create the dcp.tu56 image that hosts the
# DCP Disassembler
# We build with the OS8_TOOLTIME packs: v3d-patched.rk05

mount rk0 $os8mo/v3d-patched.rk05 required scratch
mount dt0 $os8mo/dcp.tu56 new
boot rk0

os8 ZERO DTA0:

# Copy source and doc files into the tape image.
cpto $src/src/dcp/DCP.WU DTA0:
cpto $src/src/dcp/DCP16.BN DTA0: /I
cpto $src/src/dcp/DCP24.BN DTA0: /I

os8 LOAD DTA0:DCP16.BN
os8 SAVE DTA0:DCP16.SV

os8 LOAD DTA0:DCP24.BN
os8 SAVE DTA0:DCP24.SV
